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C:\Users\Administrator>telnet 192.168. 1.1
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Velcome Visiting Huawei Home Gateway
Copyright by Huawei Technologies Co., Ltd.

Login:root
Password:
MYAP>su
success!
SU_¥AP>shell

BusyBox v1.26.2 (2018-02-09 11:04:09 CST) built-in shell (ash)
“Fnter 'help’ for a list of built-in commands.

profile close core dump

VAP (Dopra Linux) # cd /mnt/jtis2/
VAP (Dopra Linux) #

WAP (Dopra Linux) # o
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VAP (Dopra Linux) # vi hw_boardinfo,
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